Exact Audio Copy V1.0 beta 3 from 29. August 2011

EAC extraction logfile from 1. June 2012, 20:53

Tri-Synthesis / 回帰

Used drive  : TSSTcorpCDDVDW SH-S222A   Adapter: 0  ID: 0

Read mode               : Secure
Utilize accurate stream : Yes
Defeat audio cache      : No
Make use of C2 pointers : No

Read offset correction                      : 6
Overread into Lead-In and Lead-Out          : No
Fill up missing offset samples with silence : Yes
Delete leading and trailing silent blocks   : No
Null samples used in CRC calculations       : Yes
Used interface                              : Native Win32 interface for Win NT & 2000

Used output format : Internal WAV Routines
Sample format      : 44.100 Hz; 16 Bit; Stereo


TOC of the extracted CD

     Track |   Start  |  Length  | Start sector | End sector 
    ---------------------------------------------------------
        1  |  0:00.00 | 46:00.00 |         0    |   206999   


Range status and errors

Selected range

     Filename C:\Documents and Settings\Administrator\Desktop\Tri-Synthesis - 回帰.wav

     Peak level 100.0 %
     Extraction speed 11.0 X
     Range quality 100.0 %
     Copy CRC 36EB8F46
     Copy OK

No errors occurred

End of status report

==== Log checksum 4B792FB4513906596AD55FA641D49304D12207B23DE05909A6331A3CCAAD287E ====
