Exact Audio Copy V1.0 beta 3 from 29. August 2011

EAC extraction logfile from 1. June 2012, 21:03

Tri-Synthesis / Reflect

Used drive  : TSSTcorpCDDVDW SH-S222A   Adapter: 0  ID: 0

Read mode               : Secure
Utilize accurate stream : Yes
Defeat audio cache      : No
Make use of C2 pointers : No

Read offset correction                      : 6
Overread into Lead-In and Lead-Out          : No
Fill up missing offset samples with silence : Yes
Delete leading and trailing silent blocks   : No
Null samples used in CRC calculations       : Yes
Used interface                              : Native Win32 interface for Win NT & 2000

Used output format : Internal WAV Routines
Sample format      : 44.100 Hz; 16 Bit; Stereo


TOC of the extracted CD

     Track |   Start  |  Length  | Start sector | End sector 
    ---------------------------------------------------------
        1  |  0:00.00 |  6:38.00 |         0    |    29849   
        2  |  6:38.00 |  4:36.00 |     29850    |    50549   
        3  | 11:14.00 |  5:05.00 |     50550    |    73424   
        4  | 16:19.00 |  4:52.00 |     73425    |    95324   
        5  | 21:11.00 |  4:33.00 |     95325    |   115799   
        6  | 25:44.00 |  9:42.00 |    115800    |   159449   
        7  | 35:26.00 |  5:26.00 |    159450    |   183899   


Range status and errors

Selected range

     Filename C:\Documents and Settings\Administrator\Desktop\Tri-Synthesis - Reflect.wav

     Peak level 100.0 %
     Extraction speed 10.9 X
     Range quality 100.0 %
     Copy CRC EA2A38E7
     Copy OK

No errors occurred

End of status report

==== Log checksum C9587531EEC15EC5CC685F1200F4319FFD1EBD0DBBB954A80B82466379D1037A ====
